MCH Jobsite Cleanliness & Presentation Standards


Standard of Care
As a premier custom home builder, we maintain elevated jobsite cleanliness and organization standards throughout construction. Our objective is to operate a disciplined, well-managed site that reflects the quality of the finished home.

While construction environments cannot be dust-free, our sites are managed to reflect professionalism, order, and control at all times.

Clean Site Commitment
We maintain the following standards:

- Clearly designated material staging zones
- MCH supplied trash can on site
- Clear signage posted outside 
- Silt fence installed and maintained around property  
- Daily material consolidation
- Dumpsters/trailers emptied as needed to prevent overflow
- Organized storage of tools and equipment
- Defined access pathways kept clear
- Daily debris and trash removal 
- Protection of installed finishes immediately upon completion
- MCH signage is clean and straight 
-a Jobsite permit/contact board is clean and straight 


Subcontractors are required to leave the site broom-clean at the end of the day.

Daily Jobsite Expectations
At the end of each workday:

- Major debris will be placed in designated containers
- Loose trash will be thrown away
- Check neighboring properties daily for trash 
- Sweep off street in front of house and neighboring properties 
- Materials will be stacked neatly and safely
- Tools will be consolidated and secured
- Temporary coverings will be re-secured
- Access points will be clear and safe. They will also be secured every day 
-a Dumpsters and portable toilets actively maintained to prevent overflow


A luxury build requires discipline, and our trades are held to that standard.

Zero-Tolerance Policies
The following are not acceptable on our jobsites:

- Trash accumulation beyond designated areas
- Food or drinks in home 
- Unsecured materials
- Damage to installed finishes due to negligence
- Subcontractors leaving without cleaning up 

Trades who do not meet cleanliness standards may be removed from the project and/or required to pay for clean up. 


Client Site Visit Presentation
When clients visit the site, they can expect:

- An organized site
- No trash in home
- Exterior material stacked neatly 
- Interior finishes protected 
- Clear walkways into home and throughout 
- Interior safety rails up stairs (Or permanent)
- Elevators blocked off and safety nets installed
- Exterior safety rails in place (Or permanent)
- Broom swept home


Exterior Site Management
Exterior cleanliness standards include:

- Debris not allowed to migrate into neighboring lots
- Scheduled scrap removal
- Organized lumber and material stacking
- Construction silt fencing around entire lot 
- Construction driveway installed and maintained 
- Driveway and street areas cleared of excessive debris
- Street swept or blown off daily 
- Nail and fastener magnet sweeps at major phases
- Exterior safety rail installed immediately after deck fascia 
- Jobsite sign posted with No Trespassing sign, No Smoking sign, Permit, PM Contact Info, and House Address 
- Marnie Custom Home sign posted at street on opposite side as porta pot
- Fork lift parked on our property every day 

We operate with consideration for both client property and neighboring homes.


Dust Management Standards
While dust is inherent in construction, we implement:

- Controlled cutting areas when feasible – Not in screen porches
- Shop vac usage during interior cutting
- Temporary plastic barriers during heavy sanding phases
- HVAC to be turned off when sanding/cutting/spraying paint 
- Scheduled interior sweeps
- Professional cleaning a minimum of two times prior to move in 
- Project manager to have shop vac on site and use daily 

Clients should expect managed dust — not uncontrolled accumulation.



Interior Protection Protocol
As the home progresses, protective measures increase:

- Ram board floor protection installed after flooring 
- Ram board tread protection installed after finished stair treads 
- Cabinet protection upon installation
- Countertop covering until turnover
- Temporary door locks installed to secure home
- Door edge and jamb protection where necessary
- HVAC filters monitored and replaced as needed
- Post signage for no shoes in house and supply booties
- House will be swept or vacuumed daily 
- Tubs to be protected with foam board from after install until final clean 
- Doors and windows will be shut and locked everyday by MCH personal 
- Post drywall PM will designate one room for work room and store electrical fixtures, plumbing fixtures, hardware, etc. This room will have a door and a lock
- Build trim rack in garage to store trim after 1st trim. After 2nd trim anything left will be returned 
- Floor coverings will be removed after final paint and no shoes will be allowed in house 

No finished surface is left unprotected during active construction.

Scheduled Professional Cleanings

- 1st clean after countertops – pull window plastic, clean all cabinets, vacuum, mop, and wipe down bathrooms
- Clean after floor coverings are pulled 
- Power Wash exterior including all decks and garages 
- Final deep clean prior to homeowner orientation

Final Turnover Standard
Prior to homeowner orientation, the home will receive:

- Full professional interior cleaning
- Removal of protective coverings
- Debris removal from site
- Removal of portable toilet and dumpster 




